INTERMEDIATE SAILING MST 214a
1ST MIDTERM REVIEW 
 TRUE/FALSE
1.
The most important job when gybing 

2.
The command falling off 
3.
The port side running light

4.
To reef 

5.
Heeling more than 20° 

6.
The primary purpose of the keel

7.
The command 'coming about' or 'cut' should be given

8.
A westerly wind 

9.
The main halyard is generally located

10.
Sails are driven by ? wind

11.
Knots -- miles per hour.

12.
A bowline is used to tie ? loop

13.
If a person falls overboard while you’re sailing upwind vs downwind

14.
In light breezes, a normally rigged boat will sail faster

15.
The reason you avoid using seawater on an alcohol stove fire
MULTIPLE CHOICE
1.
Weather Helm is:

2.
Three techniques for stopping a boat under sail.

3.
The quickest maneuver to recover an MOB while sailing directly downwind:

4.
What would be the minimum scope for anchoring 

5.
What makes an intentional gybe safer than an accidental gybe?

6.
The steps in reefing the main 

7.
The most important job in coming about
SHORT ANSWER 
1.
 The term luffing 
2.
 No aerodynamic lift?

3.
How many life jackets are required

4.
Difference between gybing and coming about?

5.
Precisely when should you give the command of execution ?

6.
When you stop your engine to begin sailing, what steps should be taken with the control systems?

7.
What is the knee jerk reaction for man overboard recovery?

8.
You are on a run, the jib looks like it is luffing behind the main.

9.
Changing course upwind from a beam reach to a close reach is called?

10.
What is the difference between falling off and gybing?

11.
In reefing, what would be the reason for tying off both the tack and clew before raising the sail?

12-14.
Knots:

bowline, 
tautline hitch

reef knot w/ release

cleat hitch
figure 8.
