Bow person to helmsman for both dropping and picking up an anchor:

	Direction
	Arm and hand extended, pointing in the desired direction

	Increase throttle
	Fist with thumb up

	Decrease throttle
	Fist with thumb down

	Engine in neutral
	Fist

	Increase speed of boat
	Thumb up, extended arm and hand in desired direction

	Decrease speed of boat
	Thumb down, extended arm and hand in desired direction

	Stop boat’s movement
	Hand held flat palm down and moving back and forth


Bow person to helmsman for dropping an anchor:

	What is depth?
	Hand flat open with palm up

	Dropping anchor
	Index finger pointing down

	Back down on anchor to set
	Both hands palm open in back up signal

	Anchor set and holding
	OK symbol with thumb and index finger


Bow person to helmsman for picking up an anchor:

	Raising rode
	Index finger pointing up

	Anchor broken free, raising anchor
	Index finger pointing up making small circles

	Anchor up, free to maneuver boat
	open palm, waving hand in a circle point forward


Helmsman to bow person:

	Depth of water
	# of feet = # of fingers raised x 10

	Drop anchor now
	Index finger pointing down

	Anchor set and holding
	OK symbol with thumb and index finger


