Steps for dropping anchors - bow and stern: 
· Survey the anchorage

· Do the math (determine amount of rode for stern and bow according to appropriate scope)

· Measure out bow and stern rode

· Lower the stern anchor first

· Set the stern anchor

· Pay out extra stern rode to get to chosen bow anchor spot

· Lower bow anchor

· Back up, paying out bow rode until measured amount is down, while pulling in extra stern rode

· Set and test the bow anchor

· Pull in any remaining stern rode to put boat tautly between the two set anchors w/out extra play in the rode for lateral movement 

Steps for picking up anchors - bow and stern: 
· Pay out extra bow rode to back down on stern anchor

· Pull in stern rode while backing down

· Pull up stern anchor

· Proceed forward toward bow anchor while pulling in bow rode

· Pull up bow anchor 
